For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Remove the automatic transmission control lever handle.
3. Remove the console.
4. Remove the range select lever cable from the automatic transmission control.
5. Remove the electrical connector.
6. Remove the automatic transmission control bolts.
7. Remove the automatic transmission control.

### Installation Procedure

1. Install the automatic transmission control.
2. Install the automatic transmission control bolts.
3. Install the electrical connector.
4. Install the range select lever cable to the automatic transmission control.
5. Install the console. Refer to Console in Instrument Panel, Gauges and Console.
6. Install the automatic transmission control lever handle.
7. Connect the negative battery cable.