For 1990-2009 cars

# CREAK CONDITION, FRT. SEATS INSTALL NEW DERLIN PIVOT BUSH.

#### SUBJECT: BUCKET FRONT SEAT CREAK CONDITION DUE TO SPACE BETWEEN PIVOT PIN AND BUSHING (INSTALL SPACER)

#### MODELS AFFECTED: 1992 SKYLARKS WITH AR9 BUCKET SEATS

This bulletin supersedes Bulletin 92-10-38. Please discard 92-10-38.

#### CONDITION:

--------- Some owners of 1992 Skylarks with AR9 bucket front seats may comment that when making a sharp right or left turn, a creaking noise from the driver seat, and front passenger seat (when occupied) occurs.

#### CAUSE:

----- Excessive space between the inner front seatback pivot pin and the pivot bushing.

#### CORRECTION:

---------- 1. Put seatback in its most forward position.

2. From rear of seat, install spacer GM P/N 16743252 on pivot pin.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation No.: T-1818

Labor Time: 0.2 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.