For 1990-2009 cars

# OIL CANNING FLOOR PANS REPAIR PROCEDURE

SOME 1982 "A" AND "X" CAR FLOOR PANS MAY EXHIBIT AN "OIL CANNING" CONDITION IN THE FRONT AND/OR REAR FOOTWELL AREAS. THIS CONDITION, IF ENCOUNTERED, CAN BE CORRECTED BY FOLLOWING THE PROCEDURE OUTLINED BELOW. PROCEDURE 1.OPERATE FRONT SEAT INTO THE FULL REARWARD POSITION. 2.LOCATE AREA OF "OIL CANNING" BY APPLYING HAND PRESSURE ACROSS THE FRONT FOOTWELL AREA OF THE FLOOR PAN. 3.WITH FLOOR CARPET IN PLACE, USE A SUITABLE TOOL (SUCH AS A BLOCK OF WOOD) AND (SWAGE) FLOOR PAN DOWNWARD UNTIL THE "OIL CANNING" CONDITION IS ELIMINATED. 4.OPERATE FRONT SEAT INTO THE FULL FORWARD POSITION AND REPEAT STEPS 2 AND 3 FOR REAR FOOTWELL AREA. FOR WARRANTY PURPOSES, USE AN APPROPRIATE LABOUR OPERATION NUMBER FOR .2 HOURS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.