For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
A/C Refrigerant Pressure Sensor | 5 | -- | 44
Camshaft Position (CMP) Sensor Retaining Bolt | 10 | -- | 90
Crankshaft Balancer Bolt | 150 +76° | 110 +76° | --
Crankshaft Position (CKP) Sensor Bolts | 30 | 21 | --
Engine Coolant Temperature (ECT) Sensor | 23 | 17 | --
Engine Oil Level Switch | 22 | 17 | --
Exhaust Gas Recirculation Valve to Throttle Body Adapter Bolts | 30 | 22 | --
Fuel Rail Attaching Nuts or Bolts | 10 | 7 | 89
Fuel Tank Filler Pipe EVAP Pipe Hose Clamp | 2.5 | -- | 22
Fuel Tank Filler Pipe Hose Clamp | 2.5 | -- | 22
Fuel Tank Retaining Strap Bolts | 48 | 35 | --
Heated Oxygen Sensor(s) | 41 | 30 | --
Idle Air Control Valve Attaching Screws | 3 | -- | 27
Ignition Coil to Ignition Control Module Screws | 4.5 | -- | 40
In-Pipe Fuel Filter Outlet Nut | 30 | 22 | --
Knock Sensor | 19 | -- | 14
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 3 | -- | 27
Throttle Body Retaining Nuts or Bolts | 28 | 21 | --
Throttle Position Sensor Screws | 2 | -- | 18
Transaxle Range Switch Attaching Bolts | 28 | 20 | --
Upper Intake Manifold Studs or Bolts | 25 | 18 | --