For 1990-2009 cars

# RUMBLE /VIBRATION FRONT END NEW TIE ROD ASSEMBLY

CONDITION

Some 1980 and 1981 Skylarks may experience a rumbling type noise in the front end of the vehicle while driving on rough roads, or a vibration in the floor pan area at the drivers feet.

CORRECTION

A new type tie rod assembly has been developed to correct this condition. This tie rod assembly can be identified by the four (4) notches in the housing (fig. 1). The tire rod assembly is included in kit part number 7843301, (available thru WDDGM). It will be necessary to replace both left and right tie rod assemblies (2 kits) to correct this condition. Refer to fig. 2 for tie rod assembly installation procedure. Instructions are also furnished with the kit.

WARRANTY INFORMATION

Part Operation Number Labor Time Count Failed Part Trouble Code ---------------- ----------- ----- ------------ ------------ E8047 Refer to Labor 2 7832645 (1980 92 Time Guide 2 7836678 (1981) 92 Applicable Time Allowances

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.