For 1990-2009 cars

## Exhaust Manifold Removal Left Side

1. Remove the exhaust manifold heat shield bolts.
2. Remove the exhaust manifold heat shield.
3. Remove the exhaust manifold retaining nuts.
4. Remove the exhaust manifold.
5. Remove the exhaust manifold gasket.

## Exhaust Manifold Removal Right Side

1. Remove the exhaust crossover heat shield.
2. Remove the crossover pipe at the exhaust manifold.
3. Remove the heated oxygen sensor.
4. Remove the EGR pipe at the exhaust manifold.
5. Remove the exhaust pipe from the converter flange.
6. Support the converter aside.
7. Remove the converter heat shield from the vehicle body.
8. Remove the exhaust manifold heat shield fasteners.
9. Remove the exhaust manifold heat shield.
10. Remove the exhaust manifold nuts.
11. Remove the exhaust manifold.
12. Remove the exhaust manifold gasket.
13. Clean the mating surfaces at the cylinder head and at the exhaust manifold.