For 1990-2009 cars

# RTV SEALANT REPLACEMENT REPAIR VALVE COVER OIL LEAKS

#### Models Affected: 1980-1984 Skylark and Century

A new composition gasket, P/N 14089252, is available for servie use on the above 2.8L V-6 engines.

This gasket replaces the RTV sealant and is to be used for repair of rocker arm cover oil leaks and general service work.

A small amount (dab) of GM sealer must be applied at the cylinder head intake manifold split line prior to the gasket installation.

The rocker arm - cover attaching bolts must be torqued to 8.5 to 10 N.m (75-90 in. lbs.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.