For 1990-2009 cars

# WHEEL ALIGNMENT SPECIFICATION CORRECTION

#### MODELS AFFECTED: 1982 And 1983 Sklarks and Centurys

Please revise the toe-in specification shown in the Chart on Page 3A-3. Section 3A of the 1982 Skylark/Century Service Manual, and Page 3A-6, Section 3 of the 1983 Service Manual as shown below:

Camber ** 0 deg. +/- .50 deg.

Toe-In mm (per wheel) 0mm +/- 0.5 mm Deg (per wheel) 0 deg. +/- .50 deg.

Make a note of this change in your copy of the Shop Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.