For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Loosen the oil pan bolts.
3. Drain the oil.
4. Remove the oil pan attaching bolts.
5. Remove the oil pan.
6. Remove the oil pan gasket.

### Installation Procedure

1. Install the oil pan gasket. If the sealing ribs are damaged, use a new gasket.
2. Install the oil pan.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the oil pan attaching bolts.

Tighten
Tighten the oil pan bolts to 14 N·m (124 lb in).

4. Lower the vehicle.
5. Refill the transmission to the proper level with DEXRON® III oil.
6. Inspect the oil pan gasket for leaks.