For 1990-2009 cars

1. Install the ignition lock actuator assembly (4).
2. Install the lock bolt assembly (3).
3. Install the lock bolt support bracket (2).
4. Install the 2 tapping screws (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

5. Install the upper tilt head components assembly. Refer to Steering Column Tilt Head Housing - Assemble - Off Vehicle .