For 1990-2009 cars

# REAR CONTROL ARM BUSHING TOOL NUMBER REVISION

#### VEHICLES AFFECTED: 1982-84 'A' Series Vehicles 1980-84 'X' Series Vehicles

When removing or installing a control arm bushing on 1980-84 'X' series vehicles or 1982-84 'A' series vehicles use tool no. J-9519-23 in place of J-9519-10.

Please update the appropriate page of the 1984 Service Manuals listed below.

Division Section/Page -------- ------------ Chevrolet 3D-5 Pontiac 3D-5 Oldsmobile 3D-7 Buick 3D1-7

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.