For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the hydraulic system. Make a pressure test with J 5176-D . Refer to the Power Steering System Test Procedure. Does the pressure reading indicate a problem? | -- | Go to Step 2 | --
2 | Check for improper rack bearing preload. Is the rack bearing preload appropriate? | -- | Go to Step 3 | Go to Steering Gear Rack Bearing Preload Adjustment - Off Vehicle in Power Steering System
3 | Check for a bind or a catch in the steering gear. Is there a bind or a catch in the steering gear? | -- | Go to Steering Gear Replacement in Power Steering System | Go to Step 4
4 | Check for a pinched hose or line. Is a hose or a line pinched? | -- | Go to Power Steering Pressure Hose Replacement in Power Steering System | Go to Step 5
5 | Check for proper positioning of the intermediate shaft boot. Is the intermediate shaft boot positioned properly? | -- | System OK | Go to Intermediate Steering Shaft Replacement in Steering Wheel and Column-Standard