For 1990-2009 cars

# SMU - Revised DTC 0341

Subject: | Revised DTC 0341

Models: | 1996 Buick Century, Regal, Skylark

| 1996 Chevrolet Beretta, Corsica, Lumina, Monte Carlo

| 1996 Oldsmobile , Achieva, Cutlass Ciera, Cutlass Supreme

| 1996 Pontiac Grand Am, Grand Prix

| with 3.1L Engine (VIN M -- RPO L82)

This bulletin is being issued to revise Step 7 of DTC P0341 in the Engine Controls sub-section of the Service Manual. Please replace the current information in the Service Manual with the following information.

The following information has been updated within SI. If you are using a paper version of this Service Manual, please make a reference to this bulletin on the affected page.

Step 7 should read as follows: With a fused jumper connected to the sensor feed terminal, connect a DVM between the CMP sensor ground and engine ground. Does the DVM display a voltage near the specified value?