For 1990-2009 cars

### Removal Procedure

1. Remove the driver or the passenger front seat. Refer to Seat Replacement .
2. Remove the bucket or the bench seat front seatback. Refer to Front Seat Back Replacement .
3. Position the bucket or the bench seat front cushion covers (1) on a clean, dry and non abrasive surface.
4. Remove the front seat adjuster. Refer to Front Seat Adjuster Replacement or Front Seat Adjuster Motor Replacement .
5. Remove the bucket or the bench seat front cushion cover J-strips.
6. Remove the bucket or the bench seat front cushion hog rings (2).
7. Remove the bucket or the bench seat front cushion cover (1).

### Installation Procedure

1. Install the bucket or the bench seat front cushion cover (1).
2. Install the bucket or the bench seat front cushion cover J-strips.
3. Install the bucket or the bench seat front cushion cover hog rings (2).
4. Install the front seat adjuster. Refer to Front Seat Adjuster Replacement or Front Seat Adjuster Motor Replacement .
5. Position the bucket or the bench seat front cushion covers (1) on a clean, dry and nonabrasive surface.
6. Install the bucket or the bench seat front seatback. Refer to Front Seat Back Replacement .
7. Install the driver or the passenger front seat. Refer to Seat Replacement .