For 1990-2009 cars

### Removal Procedure

1. Remove the windshield side upper garnish molding. Refer to Garnish Molding Replacement - Upper in Interior Trim.
2. Remove the push pin (2) from the side roof rail weatherstrip (1).
3. Pull the top of the roof rail weatherstrip (1) away from the body flange.
4. Remove the retainer screws (2) from the roof rail weatherstrip.
5. Remove the retainer (1) from the roof rail weatherstrip.

### Installation Procedure

1. Install the retainer (1) to the side roof rail weatherstrip.
2. Install the retainer screws (2) to the roof rail weatherstrip.
3. Push the roof rail weatherstrip (1) to the body flange.
4. Install the push pin (2) to the roof rail weatherstrip (1).
5. Install the windshield side upper garnish molding. Refer to Garnish Molding Replacement - Upper in Interior Trim.