For 1990-2009 cars

#### C1 TRANSAXLE RANGE SWITCH

Connector Part Information |

• | 12129840

• | C2; TRANSAXLE RANGE SWITCH (LT GRY)

• | METRI-PACK F, SERIES 150

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 1786 | TRANSAXLE PARK/NEUTRAL SIGNAL
B | PNK | 439 | FUSE OUTPUT-IGNITION 1-TYPE III FUSE
C | GRN LT | 275 | TRANSAXLE M0UNTED NEUTRAL SAFETY SWITCH OUTPUT-PARK
D | BLK/WHT | 451 | GROUND
E | PPL | 6 | STARTER SOLENOID FEED
F | GRN LT | 24 | BACK-UP LAMP FEED
G | YEL | 5 | IGNITION SWITCH OUTPUT-CRANK

#### C2 TRANSAXLE RANGE SWITCH

Connector Part Information |

• | C1; 12191757

• | TRANSAXLE RANGE SWITCH (MD GRA)

• | METRI-PACK F, SERIES 150, 280

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | TRANSAXLE POSITION SWITCH SIGNAL - PARITY BIT
B | YEL | 772 | TRANSAXLE POSITION SWITCH SIGNAL - BIT 2
C | GRA | 773 | TRANSAXLE POSITION SWITCH SIGNAL - BIT 3
D | BLK/WHT | 771 | TRANSAXLE POSITION SWITCH SIGNAL - BIT 1