For 1990-2009 cars

# REVISED POWER STEERING ADJUSTMENT AND INSTALLATION

#### MODELS AFFECTED: All Centurys and Skylarks

The following revisions have been made to the rack bearing installation procedure on all Centurys and Skylarks with power steering:

After installing the rack bearing, turn the adjuster plug clockwise until it bottoms, then back off plug 1/8 to 1/4 turn (45 DEG to 90 DEG). The torque on the pinion must be checked and should not exceed 25 in. lbs. 2.8 N.m).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.