For 1990-2009 cars

# SHIFT LEVER RATTLE/BUZZ NOISE IN 3RD. OR 4TH. GEARS ISUZU

TRANSMISSION APPLICATIONS: SUBJECT:

1985-89 ISUZU MANUAL TRANS. SHIFT LEVER RATTLE OR BUZZ NOISE (RPO MK7, MR3, MTZ) IN 3RD OR 4TH

TRANSMISSION MODELS: VEHICLE APPLICATIONS:

ALL 1985-1989 J,L,N & P CARS

#### Bulletin Covers:

This bulletin is being issued to supersede Bulletin 86-7050-104, all copies of this bulletin should be destroyed.

Some 1985-89 J, L, N, and P cars equipped with Isuzu 5-Speed manual transaxles may exhibit a rattle or buzzing type noise through the shifter handle while driving in 3rd or 4th gears. This noise condition is normally caused by a run-out condition between the 3-4 synchronizer and the 3rd or 4th input gears.

This condition has been corrected during the 1989 model year. Therefore any 1989 vehicle equipped with an Isuzu unit built on or after serial number IX17J01 should not have this condition. The serial number is printed on the transmission bar code label, which is located on the clutch housing. The serial number should be read as follows:

Positions l.........Corp. Name (i.e. I = Isuzu) 2.........Month of build 1-9, X, Y, or Z (i. e. 2 = Feb., 7 = July, X = Oct., Z = Dec.) 3,4.......Day of month built 1-31 (i. e. 17 = 17th day of the month) 5.........Year of build (i.e. J-Z = 1988, A-I = 1989)

Examples: Unit IX17JOl = built on Oct. 17, 1988. Unit I13OB35 = built on Jan. 30, 1989.

To repair this condition install a new 3rd/4th synchronizer assembly, 3rd/4th fork assembly, and a 3rd or 4th input gear. Refer to the following chart when ordering parts from CANSPO.

DESCRIPTION DIVISION BODY ENGINE MODEL PART ----------- -------- ---- VIN YEAR NUMBER --- ---- ------ Fork - 3rd/4th All All All All 94464752 Synchronizer Asm. All All All All 94249573 - 3rd/4th 3rd Input Gear Olds/Bui/Chev/Cad J 1 88-89 94149668 Olds/Bui/Chev/Cad J P,1 85-87 94139574 Pont/Olds/Bui J K,O 85-89 94149668 Pont/Olds/Bui N U 85-89 94149668 Pont P R 85-89 94149668 Chev L 1 88-89 94139574 4th Input Gear Olds/Bui/Chev/Cad J 1 88-89 94139575 Olds/Bui/Chev/Cad J P,1 85-87 94139576 Pont/Olds/Bui J K,O 85-89 94139575 Pont/Olds/Bui N U 85-89 94139575 Pont P R 85-89 94139575 Chev L 1 88-89 94139576

Use applicable Labour Operation Number and Time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.