For 1990-2009 cars

# RT. FRONT CARPET WET DUE TO WATER LEAK

#### SUBJECT: RIGHT FRONT CARPET WET DUE TO WATER LEAK BETWEEN AIR INLET SCREEN AND WINDSHIELD (INSTALL SEALING STRIP)

#### MODELS: 1991-94 BUICK SKYLARK 1991-94 CHEVROLET BERETTA AND CORSICA 1991 OLDSMOBILE CUTLASS CALAIS 1992-94 OLDSMOBILE ACHIEVA 1991-94 PONTIAC GRAND AM

#### CONDITION:

SOME OWNERS MAY COMMENT ON THE RIGHT FRONT CARPET WET DUE TO WATER LEAK BETWEEN AIR INLET SCREEN AND WINDSHIELD.

#### CAUSE:

WATER LEAKING BETWEEN THE AIR INLET SCREEN AND WINDSHIELD ENTERS THE PASSENGER COMPARTMENT THROUGH THE HVAC AIR INLET STACK ASSEMBLY.

#### CORRECTION:

FOR BUICK, OLDSMOBILE AND PONTIAC:

1. REMOVE WINDSHIELD WIPER ARMS, REFER TO SECTION 8E OF THE APPROPRIATE SERVICE MANUAL.

2. REMOVE AIR INLET SCREEN, REFER TO SECTION 10-5 OF THE APPROPRIATE SERVICE MANUAL.

3. TRIM ENOUGH WINDSHIELD URETHANE TO INSTALL SEALING STRIP, (REFER TO FIGURE 1).

4. REMOVE BACKING PAPER FROM SEALING STRIP, P/N 22639153, AND INSTALL SEALING STRIP, (REFER TO FIGURE 1).

5. INSTALL AIR INLET SCREEN, REFER TO SECTION 10-5 OF THE APPROPRIATE SERVICE MANUAL.

6. INSTALL WINDSHIELD WIPER ARMS, REFER TO SECTION 8E OF THE APPROPRIATE SERVICE MANUAL.

#### FOR CHEVROLET:

1. REMOVE RIGHT WINDSHIELD WIPER ARM, REFER TO SECTION 8E OF THE SERVICE MANUAL.

2. REMOVE RIGHT AIR INLET SCREEN, REFER TO SECTION 10-5 OF THE SERVICE MANUAL.

3. TRIM ENOUGH WINDSHIELD URETHANE TO INSTALL SEALING STRIP, (REFER TO FIGURE 2).

4. REMOVE BACKING PAPER FROM SEALING STRIP, P/N 22639153, AND INSTALL SEALING STRIP, (REFER TO FIGURE 2).

5. REMOVE ALL BUTYL FROM WINDSHIELD, AIR INLET SCREEN AND DASH EXTENSION.

6. APPLY BUTYL TO RIGHT AIR INLET SCREEN, REFER TO SECTION 10-5 OF THE SERVICE MANUAL.

7. INSTALL RIGHT AIR INLET SCREEN, REFER TO SECTION 10-5 OF THE SERVICE MANUAL.

8. INSTALL RIGHT WINDSHIELD WIPER ARM, REFER TO SECTION 8E OF THE SERVICE MANUAL.

PARTS ARE EXPECTED TO BE AVAILABLE ON OCTOBER 31, 1994.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: D2000 FOR CHEVROLET, USE LABOR TIME: 0.4 HR FOR BUICK, OLDS., PONTIAC, USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.