For 1990-2009 cars

# GAS SUPPORT INSTALLATION DIAMETER ROD REAR OF CAR

THIS BULLETIN IS BEING RELEASED TO INSURE GAS SUPPORTS ARE INSTALLED PROPERLY IN THE FIELD. INSTALLATION & LOCATION OF GAS SUPPORTS MODELS ALL MODELS EXCEPT "E" - "G69" (81 A-69) DECK LIDS SMALLER DIAMETER ROD IS TO BE TOWARD THE REAR OF THE CAR. HATCHES SMALLER DIAMETER ROD IS TO BE ATTACHED TO THE BODY SIDE OF THE OPENING. TAILGATES SAME AS HATCHES MODELS "E" AND "G-69" ("81" A-69) DECK LIDS SMALLER DIAMETER ROD IS TO BE TOWARD THE FRONT OF THE CAR. FOR DETAILED REMOVAL AND INSTALLATION PROCEDURES OF REAR COMPARTMENT LID GAS SUPPORT ASSEMBLIES, REFER TO SECTION 7 OF YOUR FISHER BODY SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.