For 1990-2009 cars

# WASHER PUMP INOPERATIVE WILL NOT PRIME

#### SUBJECT: WASHER PUMP INOPERATIVE - WILL NOT PRIME OR PUMP WASHER FLUID (REPLACE FILTER GROMMET)

#### MODELS: 1995 BUICK SKYLARK 1995 CHEVROLET BERETTA, CORSICA 1995 OLDSMOBILE ACHIEVA 1995 PONTIAC GRAND AM

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE WASHER PUMP MAY NOT PRIME OR PUMP WASHER FLUID.

#### CAUSE:

THE FILTER GROMMET RESTRICTS THE FLOW OF WASHER FLUID. AS THE LEVEL OF FLUID DECREASES, THE PRESSURE OF THE WASHER FLUID DECREASES TO A POINT WHERE IT DOES NOT FLOW THROUGH THE FILTER GROMMET.

#### CORRECTION:

A NEW FILTER GROMMET, P/N 22039457, MUST BE INSTALLED IN ORDER TO CORRECT THIS CONDITION. REFER TO SECTION 8E OF THE APPROPRIATE SERVICE MANUAL.

1. REMOVE THE PUMP FROM THE WASHER BOTTLE.

2. REMOVE THE FILTER GROMMET FROM THE PUMP (SEE FIGURE 1).

3. INSTALL A NEW GROMMET WITHOUT FILTER, P/N 22039457, IN THE WASHER BOTTLE.

4. INSTALL THE WASHER PUMP INTO THE NEW GROMMET AND WASHER BOTTLE (SEE FIGURE 2).

#### PARTS AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: N3860 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.