For 1990-2009 cars

# UPDATE-WHEEL ALIGNMENT CORRECT CAMBER SPECIFICATIONS

#### VEHICLES AFFECTED: 1990 "J" AND "N" MODELS

The front wheel camber specifications for the 1990 'J' and 'N' vehicles are shown incorrectly in section 3A of the 1990 Chassis Service Manual.

ALL 1990 model J/N vehicle front wheel camber specifications should be 0 degree +/- .70.

Please note this correction in your Service Manual (with reference to this bulletin) on page:

Chevrolet Cavalier 3A-7, Fig 7 Pontiac Sunbird 3A-6, Fig 7 Oldsmobile Cutlass Calais 3A-6, Fig 7 Buick Skylark 3A-6, Fig 7

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.