For 1990-2009 cars

### Removal Procedure

1. Remove the screws from the fascia.
2. Remove the bracket from the fascia.

### Installation Procedure

#### Tools Required

J 39312 Rivet Gun

1. Locate the 2 dimples on the lower portion of the fascia on the driver side. Drill 2 6-mm (0.25-in) holes.
2. Install the bracket to the fascia.
3. Install 2 pop rivets using the J 39312 or equivalent.
4. Drill 2 6-mm (0.25-in) holes in front of the fascia using the upper holes located in the pockets of the license bracket as the templates.
5. Install 2 pop rivets using the J 39312 or equivalent.