For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
2. Disconnect the harness connector.
3. Remove the two screws and the actuator.

### Installation Procedure

1. Position the actuator and install the screws.
2. Connect the harness connector.
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.