For 1990-2009 cars

### Removal Procedure

1. Disconnect the reading lamp wire from the rearview mirror, if equipped.
2. Loosen the set screw in the base of the mirror.
3. Remove the mirror from the mounting pad.

### Installation Procedure

1. Install the mirror to the mounting pad.
2. Tighten the set screw that retains the mirror base to the mounting pad.
3. Connect the reading lamp wire to the rearview mirror, if applicable.