For 1990-2009 cars

### Removal Procedure

1. Slide the sunshade assembly to the open position.
2. With the glass panel in the fully closed position, remove the 6 sunroof window screws (3 screws on each side).
3. Remove the sunroof window (4).

### Installation Procedure

1. Install the sunroof window (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 6 sunroof window screws.

Tighten
Tighten the sunroof window screws to fully drive and seat, but not strip.

3. Adjust the glass panel height. Refer to Sunroof Window Height and Opening Fit Adjustment .