For 1990-2009 cars

# 125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE

#### VEHICLES AFFECTED: 1982-84 Vehicles Equipped With THM 125/125-C Transmissions

Some 1982 thru 1984 125/125-C transmissions may exhibit a rough neutral to drive gear engagement.

Beginning December 15, 1983, a new forward clutch wave plate, part number 8652126 went into production. Refer to the chart below for model and serial number application.

When servicing any 1982 thru 1984 model THM 125/125-C transmission for this rough neutral to drive condition, order part number 8652126. Refer to the service manual tor removal and replacement of the forward clutch wave plate.

#### MODEL SERIAL NO. MODEL SERIAL No. ----- ---------- ----- ---------- CA 2724 EQ 136060 CB 221301 EW 1014 CC 1219 HC 2086 CE 77876 HM 2980 CF 7881 HP 1154 CT 4840 HS 16495 EB 3276 HX 6250 EF 7642 HY 29466 EI 6450 PD 2508 EJ 1006 PE 64573 EK 11147 PF 31776 EL 4201 PG 63043 EM 3342 PJ 8148 EN 4984 PW 82620 EP 2427

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.