For 1990-2009 cars

Angle | Alignment Specifications | Tolerance
--- | --- | ---
Front Caster (Cross) | 4.30 | +/- 1.00 Degrees
Front Camber (Cross) | 0.20 | +/- 1.00 Degrees
Individual Toe | 0.00 | +/- 0.12 Degrees
Measure the above toe angles with the steering wheel at level position, visually aligned with the column.
Sum Toe | 0.00 | +/- 0.25 Degrees
Cross Camber | 0.00 | +/- 1.00 Degrees
(Slight cross camber specification differences can be made when servicing the vehicle for steering pull.)
Cross Caster | 0.00 | +/- 1.00 Degrees
Rear Camber Cross | -0.25 | +/- 0.75 Degrees
Rear Sum Toe | 0.20 | +/- 0.30 Degrees
Rear Thrust Angle | 0.25 | +/- 0.25 Degrees