For 1990-2009 cars

# I/P AIR OUTLET DUCTS REMOVAL SERVICE MANUAL REMOVAL

#### VEHICLES AFFECTED: 1980-84 Omega

When removing the instrument panel air outlet ducts on a 1980-84 omega, it is not necessary to remove the instrument panel as noted on page 8C2-9 of the 1984 Service Manual. Follow the revised service procedure listed below.

1. Disconnect the lower instrument panel.

2. Remove the screws attaching the duct(s) to the instrument panel.

3. Remove the duct(s).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.