LOCKING FUEL FILLER DOOR INOP. RELEASE CABLE EXPLAINED. Buick Somerset 1986

For 1990-2009 cars

# LOCKING FUEL FILLER DOOR INOP. RELEASE CABLE EXPLAINED

BLOCKING FUEL FILLER DOOR WILL NOT OPEN

#### VEHICLES AFFECTED: 1985-86 'N' - Models -----------------

If subject condition is encountered due to a discontinued release cable, the fuel filler door may be opened by using the following procedure.

1. Open deck lid and pull back the right quarter trim panel of the trunk.

2. Locate the fuel filler door release cable.

3. Grasp cable just behind grommet and pull rearward.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.