OIL LEAK AT CRANKSHAFT BALANCER ASSEMBLY BOLT. Buick Somerset 1985

For 1990-2009 cars

# OIL LEAK AT CRANKSHAFT BALANCER ASSEMBLY BOLT

#### Models Affected: All 1985 and Prior Models with 3.0L (Vin Code E & L) and 3.8L (Vin Code A, 3 & 9) V6 Engines

If an engine oil leak occurs at the crankshaft balancer assembly attaching bolt on the above engines, it can be repaired by removing the bolt and replacing the washer under the bolt head with a new washer, Part number 25525918.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.