IN DOOR WATER DEFLECTOR SERVICE AND REPAIR PROCEDURE. Buick Somerset 1987

For 1990-2009 cars

# IN DOOR WATER DEFLECTOR SERVICE AND REPAIR PROCEDURE

DOOR WATER DEFLECTOR SERVICE PROCEDURE

#### VEHICLES AFFECTED: 1987 - 88 "N" CAR

The following information should be added to Section 5F in the 1987 Body Service Manual. This same statement will appear in the 1988 Body Service Manual.

"When working on any door component which requires partial or complete removal of the water deflector, any damage caused to the water deflector or any original holes in the deflector which do not line up with fastener locations in the door inner panel or if the adhesive loses it's effectiveness, it must be repaired by applying waterproof tape to the affected area of the water deflector prior to installing the door trim panel. This is essential to prevent water entry into the passenger compartment and to maintain original sealing integrity."

Leaks past the water deflector can be difficult to locate as they only appear in the foot well area of the car. Be sure to check the lower edge of the door trim panels during water test when checking for unexplained water accumulation in the floor pan area.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.