A/C ADAPTORS FOR HIGH FILL RATE SCHRADER-TYPE VALVES. Buick Somerset 1986

For 1990-2009 cars

# A/C ADAPTORS FOR HIGH FILL RATE SCHRADER-TYPE VALVES

#### VEHICLES AFFECTED: 1986 - 'N' Series

There are some car models that use a high fill rate Schrader-type valve that contains a different valve. This valve requires a depressor that will depress it deeper before the valve will open. This valve can be identified by looking into the opening. The depressor for the high flow valve is about three times as long as the older valve. It also has a spring wound around it, while the older valve does not. Kent-Moore has the following, adaptors for service use.

J25498-A Straight Brass Adaptor - For use with both valves.

J25499-A 90 Degree Brass Adaptor - For use with both valves.

J34122-A 6 in. Flexible Adaptor For use in both valves.

J25498-2A Valve, Depressor - Will convert older adaptors for use with both valves.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.