EXCESSIVE SPARK KNOCK -PING INOPERATIVE EGR VALVE. Buick Somerset 1986

For 1990-2009 cars

# EXCESSIVE SPARK KNOCK -PING INOPERATIVE EGR VALVE

#### VEHICLES AFFECTED: 1986 'A-F-N-P CARS, S/T TRUCKS AND 'M' VANS WITH 2.5L L4 ENGINE; RPO LR8, LQ9, L68, LN8

Some 1986 vehicles with a 2.5L L4 engine may exhibit excessive spark knock, at part throttle, due to an inoperative EGR valve.

If an EGR valve has been diagnosed as inoperative because it does not respond to a normal vacuum signal, remove the vacuum hose and check the orifice in the vacuum fitting for a plugged condition (See Figure 1). Orifice inside diameter is .040" to .050".

The orifice may have excessive, hardened hose assembly lubricant blocking it. If this condition exists, clear the orifice with a small wire, or pin, return the vacuum hose to the fitting and test the EGR valve for function.

If the EGR is still inoperative, replace it.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.