ROCKER COVER AND/OR GASKET REPLACEMENT LABOR OPERATIONS. Buick Somerset 1985

For 1990-2009 cars

# ROCKER COVER AND/OR GASKET REPLACEMENT LABOR OPERATIONS

THE FOLLOWING LABOR OPERATIONS HAVE BEEN REVISED, EFFECTIVE IMMEDIATELY. THE NEW TIMES ARE:

COVER AND/OR GASKET, ROCKER - REPLACE

J0300 RIGHT BANK .9 HRS. J030L LEFT BANK .2 HRS. J0307 BOTH BANKS 1.0 HRS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.