CRANKSHAFT SENSOR ATTACHING BOLT INSTALLATION- TORQUE. Buick Somerset 1985

For 1990-2009 cars

# CRANKSHAFT SENSOR ATTACHING BOLT INSTALLATION- TORQUE

#### Models Affected: 1985 Somerset Regals Equipped with 3.0L MFI Engine (Vin Code L)

the correct installation torque of the two crankshaft sensor to front cover attaching bolts is 30 N.m (22 lb. ft.). Figure 19, on page 6A5A-10 of the 1985 Buick Chassis Service Manual should be revised to show this information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.