FRONT GRILL AIR DEFLECTOR REPLACE IF WARPED/DISTORTED. Buick Somerset 1987

For 1990-2009 cars

# FRONT GRILL AIR DEFLECTOR REPLACE IF WARPED/DISTORTED

#### VEHICLES AFFECTED: 1987 CALAIS

Some 1987 Calais models may experience a warped/distorted front grille air deflector. To correct this condition it will be necessary to replace the air deflector and secure as follows. Refer to illustration.

1. Discard two indicated attaching screws,

2. Starting from the center, seat (do not strip) the remaining attachment screws.

3. Back out (loosen) each screw except Screw "A" 3/4 to 1 turn from the seated position. Screw "A" should remain tight.

This process will allow the air deflector matieral to expand/contract due to changing enmvironment conditions without damage.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.