INFORMATION ON FUEL INJECTION HARNESS REPAIR. Cadillac Allante 1993

For 1990-2009 cars

# INFORMATION ON FUEL INJECTION HARNESS REPAIR

REPAIR OF FUEL INJECTION WIRING THAT IS LOCATED UNDER THE INTAKE MANIFOLD COVER ON 1993 E, K, AND V CARS WITH 4.6L ENGINES IS BY HARNESS REPLACEMENT ONLY. THE FUEL INJECTION WIRING HARNESS PART NUMBER IS 12121298 AND IS CURRENTLY AVAILABLE FROM GMSPO.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FOR WARRANTY PURPOSES USE LABOR OPERATION J5660 AT .9 HOUR (RAIL, FUEL-REPLACE) WHEN REPLACING THE FUEL INJECTION WIRING HARNESS.

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.