SOFT TOP MATERIAL WEAR FROM RUBBING ON STOWAGE COVER. Cadillac Allante 1990

For 1990-2009 cars

# SOFT TOP MATERIAL WEAR FROM RUBBING ON STOWAGE COVER

#### SUBJECT: SOFT TOP MATERIAL WEAR FROM RUBBING ON STOWAGE COVER (APPLY SQUEAK REDUCTION TAPE)

#### VEHICLES AFFECTED: 1990-92 "V" MODELS

Some 1990 (with RPO V4J) - 1992 Allantes may exhibit wear of the soft top material above the quarter windows (often most pronounced on the fabric bead). Refer to Figure 1. This condition is caused by the top material rubbing on the bottom side of the stowage cover when the top is in the stowed position. To repair this condition use the following service procedure:

1. Inspect the bottom side of the soft top stowage cover for polished spots indicating wear areas. Refer to Figure 2.

2. Apply 3M No. 5430 squeak reduction tape, or equivalent, on the bottom side of the stowage cover, completely covering suspected contact points. Refer to Figure 3.

If vehicle is being repaired under warranty use: .2 hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.