DOOR WILL NOT OPEN WITHIN SIDE DOOR HANDLE (REPL. HANDLE). Cadillac Allante 1993

For 1990-2009 cars

# DOOR WILL NOT OPEN WITHIN SIDE DOOR HANDLE (REPL. HANDLE)

#### SUBJECT: DOOR WILL NOT OPEN WITH INSIDE DOOR HANDLE (REPLACE HANDLE ASSEMBLY AND ROD)

#### MODELS: 1993 CADILLAC ALLANTE

#### CONDITION:

SOME OWNERS MAY EXPERIENCE A CONDITION WHERE THE DOOR WILL NOT OPEN USING THE INSIDE DOOR HANDLE IN WARM WEATHER.

#### CAUSE:

MATERIAL DEFORMATION DOES NOT ALLOW THE INSIDE DOOR HANDLE TO ACTIVATE THE ROD WITH FULL HANDLE TRAVEL.

#### CORRECTION:

REPLACE THE INSIDE DOOR HANDLE ASSEMBLY AND THE INSIDE DOOR HANDLE ROD WITH THE UPDATED PARTS LISTED BELOW. THE NEW ROD HAS A LARGER DIAMETER AND ADDITIONAL THREADS FOR ADJUSTMENT. THE MATERIAL IN THE HANDLE ASSEMBLY HAS BEEN REVISED.

DESCRIPTION PART NUMBER QTY

ROD, DOOR INSIDE HANDLE 3544862 1/DOOR

HANDLE ASSEMBLY MAROON 3545029 - RH 1/DOOR 3545030 - LH

CHARCOAL 3545031 - RH 3545032 - LH

NATURAL BEIGE 3545033 - RH 3545034 - LH

#### SERVICE PROCEDURES:

REMOVE/DISCONNECT 1. ARMREST (2 SCREWS).

2. SWITCH PLATE. PUSH FORWARD AND LIFT UP ON REAR.

3. DOOR INSIDE HANDLE ROD AT HANDLE (ACCESS THROUGH SWITCH PLATE OPENING). ROTATE PLASTIC RETAINER OUT OF WAY AND LIFT ROD END TO DISCONNECT.

4. INSIDE DOOR HANDLE (2 SCREWS).

5. ARMREST BRACKET (4 SCREWS). DISCONNECT EXPRESS WINDOW MODULE CONNECTOR.

6. LOWER DOOR PANEL (SCREWS AT BOTTOM OF PANEL). DISCONNECT MIRROR SWITCH CONNECTOR (DRIVER'S DOOR) AND ALLOW PANEL TO DROP.

7. DOOR INSIDE HANDLE ROD.

REPLACE/CONNECT 1. DOOR INSIDE HANDLE ROD WITH NEW ROD, P/N 3544862.

2. MIRROR SWITCH CONNECTOR AND LOWER DOOR PANEL.

3. INSIDE DOOR HANDLE WITH NEW HANDLE ASSEMBLY (P/N ACCORDING TO COLOR).

4. ROD AT HANDLE AND SECURE WITH RETAINER.

5. ADJUST ROD AS SHORT AS POSSIBLE TO ELIMINATE PLAY WITHOUT PULLING ON THE DOOR INSIDE HANDLE. ACCESS THROUGH SWITCH PLATE OPENING.

6. EXPRESS WINDOW MODULE CONNECTOR AND ARMREST BRACKET.

7. ARMREST.

8. SWITCH PLATE.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION DESCRIPTION

B4368 DOOR INSIDE HANDLE/ROD - REPLACE, PASSENGER'S DOOR B4369 DOOR INSIDE HANDLE/ROD - REPLACE, DRIVER'S DOOR

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 CADILLAC MOTOR CAR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.