LOW PROFILE HEADREST REMOVAL SERVICE PROCEDURE. Cadillac Allante 1988

For 1990-2009 cars

# LOW PROFILE HEADREST REMOVAL SERVICE PROCEDURE

MODEIS AFFECTED: 1988 ALLANTES

This bulletin provides supplemental information on the low profile headrest removal and replacement for the 1987-1988 Allante Service Information Manual.

1. Raise headrest to full height position.

2. Release boot retainers and lift boots; remove shoulder belt guide.

3. Remove seat back cover.

4. Remove trim from top of seat back center cushion (four clips at back, bend two tabs at top, front) to access support retaining clips.

5. Remove clips.

6. Lift headrest to remove from seat.

Reverse procedure to reinstall headrest, ensuring that flat side of clip contacts support grooves/indentations

Use caution when reinstalling clips; a dropped clip may fall into closed bonom of seat back frame resulting in a rattle.

For warranty purposes use Labor Operations C6690 (RH) or C6691 (LH) at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.