INFO. ON TRANSAXLE OIL COOLER LINE SERVICE PRECAUTIONS. Cadillac Allante 1993

For 1990-2009 cars

# INFO. ON TRANSAXLE OIL COOLER LINE SERVICE PRECAUTIONS

#### SUBJECT: INFORMATION ON TRANSAXLE OIL COOLER LINE SERVICE PRECAUTIONS

#### VEHICLES AFFECTED: 1993 "E","K", "V" MODELS

Care must be taken to prevent twisting of the transaxle cooler pipe/hose assemblies during service procedures which may necessitate the removal or disconnection of these lines.

It is possible to cause a crimp in either oil cooler hoses while tightening the fitting. The return line assembly can also be rotated 360 degrees during installation which causes the hose material to twist and restrict the fluid flow to the transaxle.

#### NOTE: The hose sections of the return lines are protected by plastic conduits which could prevent a technician from easily seeing this condition.

The reduced fluid flow in either case can cause transaxle damage or failure.

To prevent possible damage to the transaxle after service of the cooler line:

1. Carefully hold the sending or lower pipe in place with pliers or lightly locked vise grips (take care not to crimp the pipe) to prevent rotation while tightening the fitting.

2. Peel back the conduit on the return (upper) hose and visually inspect both upper and lower hoses to detect any twisting which may have occurred. If twisting has occurred, disconnect the line and reorient the pipe to eliminate the problem. Conduit should be reinstalled once the proper orientation has been confirmed.

Refer to Section 7A, page 8 of the 1993 Allante preliminary Service Manual for illustrations and service procedures.

#### WARRANTY INFORMATION:

Operation Description Operation Vehicle Series Number E K V --------------------------------------------------------------------------- Line, Transmission/ E,K,V With K5262 1.7 1.7 1.7 Transaxle Oil Cooler 4.6L

E,K,V With 5263 0.3 0.3 0.3 4.6L

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.