CLUNK/RATTLE AT LEFT FRT. CNR. (DIAG./REPL./SECURE RTRN. LINE. Cadillac Allante 1992

For 1990-2009 cars

# CLUNK/RATTLE AT LEFT FRT. CNR. (DIAG./REPL./SECURE RTRN. LINE

#### SUBJECT: CLUNK OR RATTLE AT LEFT FRONT CORNER OF CAR (DIAGNOSE/REPLACE OR SECURE RETURN LINE)

#### MODELS AFFECTED: 1992 ELDORADOS, SEVILLES, AND ALLANTES

Some 1992 Eldorados, Sevilles, and Allantes may experience a clunk or rattle condition at the left front corner of the car due to the power steering left-hand return line contacting the transaxle case.

To repair this condition inspect the left-hand return line. If the return line shows wear as a result of the contact, it should be replaced per Service Information Manual procedures in Section 3B. If no wear is evident, secure the left-hand return line to the cradle just forward of the left transaxle mount with a plastic tie strap as shown in Figure 1. If the left-hand return line is replaced, the new line should be secured to the frame with a plastic tie strap.

For securing the line to the cradle only, use Labor Operation T6679 at .3 hour. If the left - hand return line is replaced, use Labor Operation E8625 at .8 hour for Eldorados and Sevilles or .6 hour for Allantes.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.