CONSOLE DOOR CLOSING EFFORT TRIM RUBBER BUMPER MATERIAL. Cadillac Allante 1990

For 1990-2009 cars

# CONSOLE DOOR CLOSING EFFORT TRIM RUBBER BUMPER MATERIAL

#### VEHICLES AFFECTED: 1987-1990 V

Some 1987-1990 Allantes may exhibit an excessive console door closing effort. The console door and hinge are not adjustable. Therefore, the following procedure should be used to reduce the console door closing effort:

1. Open console door.

2. Trim off 3.Omm from the rubber bumpers with a razor blade or utility knife. Refer to Figure 1.

3 Check console door closing effort.

4. If effort is still unacceptable, trim off 1.0mm additional material from rubber bumpers.

#### NOTICE: Removal of any additional material from the bumpers will not improve closing effort. Removal of additional material may introduce a rattle in the console area. Do not remove any more material after step 4 has been completed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.