POOR FIT QUARTER GLASS TO SOFT TOP. Cadillac Allante 1987

For 1990-2009 cars

# POOR FIT QUARTER GLASS TO SOFT TOP

SOFT TOP QUARTER WINDOW WEATHERSTRIP ASSEMBLY REPLACEMENT

#### VEHICLES AFFECTED: 1987 ALLANTE ------------------

Some 1987 Allantes built before VIN breakpoint 100699 may experience a poor fit of the rear door glass to the soft top quarter window weatherstrip. This condition may be caused by a "blow out" clip that is missing from the quarter window weatherstrip retainer (refer to Figure 1). To repair this condition, use the following procedure:

1. Remove the hard top and place it on a protected surface. 2. Raise the soft top boot cover. 3. Raise the soft top and latch it to the windshield header, lower soft top boot cover, and lock the rear hook into the pull down motor assembly. 4. Inspect for the "blow out" clip on the quarter window weatherstrip retainer (refer to Figure 1). 5. If there is no "blow out" clip, replace the weatherstrip assemblies as necessary with the latest design, P/N 1646627 (RH) and 1646628 (LH), by removing and installing four Phillips head screws on the inboard side of the metal weatherstrip retainer.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.