ACCEL PEDAL POSITION/COMFORT REMOVE/REINSTALL PEDAL BRKT. Cadillac Allante 1993

For 1990-2009 cars

# ACCEL PEDAL POSITION/COMFORT REMOVE/REINSTALL PEDAL BRKT

#### SUBJECT: ACCELERATOR PEDAL POSITION OR COMFORT (REMOVE AND REINSTALL PEDAL MOUNTING BRACKET)

#### VEHICLES AFFECTED: 1992-93 "E, K AND V" MODELS

#### CONDITION:

--------- Some owners of 1992 Cadillac Eldorados and Sevilles and 1993 Allantes may comment that the accelerator pedal feels off angle or is too far forward.

#### CAUSE:

----- This condition may be caused by the position of the accelerator pedal bracket.

#### NOTE: This condition does not affect accelerator pedal operation. This condition relates to pedal comfort only.

#### CORRECTION:

---------- To correct this condition use the following procedure:

1. Remove lower accelerator pedal mounting bracket screw and discard. (Refer to Figure 1.)

2. Use a screwdriver to pry the accelerator bracket away from the dash panel. Install a 7mm thick shim or washer between the lower mounting bracket and the front of dash mounting pad. (Refer to Figure 1.)

3. Install a longer screw, 10mm hex with flat washer, (M6.3 x 1.81 x 20).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.