ALLANTE CLUSTER BEZEL ITCH (INSTALL CLUSTER TRIM). Cadillac Allante 1988

For 1990-2009 cars

# ALLANTE CLUSTER BEZEL ITCH (INSTALL CLUSTER TRIM)

#### MODELS AFFECTED: 1988-1990 ALLANTES

Some 1988-1990 Allantes equipped with the analog instrument cluster may exhibit a condition of a squeak or itch noise in the instrument cluster bezel area. To repair this condition use the following procedure:

1. Remove cluster trim plate. Refer to Section 8C.

2. File down the four lower trim ramps as indicated in Figure 1.

3. Place a strip of thin, self-adhesive felt to the back side of the trim plate at the upper edge. Refer to Figure 2.

4. Install cluster trim using three washers (no greater than 2mm thick) between the cluster and trim plate as shown in Figure 3.

For warranty purposes use Labor Operation T6418 at .8 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.