WINDSHIELD WEATHERSTRIP TEARS OR SEPARATES AT UPPER CORNERS. Cadillac Allante 1987

For 1990-2009 cars

# WINDSHIELD WEATHERSTRIP TEARS OR SEPARATES AT UPPER CORNERS

#### SUBJECT: WINDSHIELD WEATHER-STRIP TEARS OR SEPARATES AT UPPER CORNERS (INSTALL NEW WEATHER-STRIP)

#### VEHICLES AFFECTED: 1987-1991 CADILLAC ALLANTE

On some 1987-1991 Allantes, the weather-strip around the perimeter of the windshield may separate or tear at the mold line near the upper corners.

To repair this condition install new design weather-strip, P/N 3535749.

This new weather-strip is 6mm longer cross car and eliminates excessive tension at the corners when installed.

For vehicles repaired under warranty use:

Labor Operation C1008 at 0.6 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.