INFORMATION ON LUBRICATION SYSTEM PRIMING PROCEDURE. Cadillac Allante 1993

For 1990-2009 cars

# INFORMATION ON LUBRICATION SYSTEM PRIMING PROCEDURE

#### SUBJECT: INFORMATION ON LUBRICATION SYSTEM PRIMING PROCEDURE

#### MODELS: 1993 CADILLAC ALLANTE 1993-94 CADILLAC ELDORADO AND SEVILLE 1994 CADILLAC CONCOURS WITH 4.6L NORTHSTAR ENGINE (RPOS LD8, L37 - VINS Y, 9)

WHEN SERVICING A 4.6L NORTHSTAR ENGINE AND OIL PUMP REMOVAL IS REQUIRED, THE FOLLOWING PROCEDURES MUST BE FOLLOWED TO PRIME THE ENGINE'S LUBRICATION SYSTEM ONCE REPAIRS ARE COMPLETED.

1. THOROUGHLY PACK THE OIL PUMP WITH AMOJELL(TM) OR WHITE PETROLEUM JELLY DURING REASSEMBLY AND **FILL** THE NEW OIL FILTER WITH CORRECT SPECIFICATION ENGINE OIL BEFORE INSTALLATION.

2. VERIFY ENGINE OIL IS AT PROPER LEVEL. SYSTEM CAPACITY IS 7 QUARTS WITH OIL FILTER FULL. FILL TO PROPER LEVEL, IF NECESSARY.

3. DISCONNECT THE RIGHT-FRONT CONNECTOR (POWER LEAD, SEE FIGURE 1) FROM THE DIS MODULE AND CRANK THE ENGINE FOR 30 SECONDS.

4. RECONNECT THE POWER LEAD TO THE DIS AND START THE ENGINE. CHECK THE DIS FOR "LOW OIL PRESSURE" MESSAGE AND LISTEN FOR ANY AUDIBLE ENGINE NOISE SUCH AS LIFTERS "TICKING."

5. IF ENGINE NOISES PERSIST, STOP ENGINE AND REMOVE THE OIL PRESSURE SWITCH FROM THE OIL FILTER ADAPTER AND INSTALL AN OIL PRESSURE GAUGE. BE CAREFUL NOT TO DAMAGE THE THREADS IN THE ADAPTER.

6. IF OIL PRESSURE IS INDICATED ON THE GAUGE AND NO UNUSUAL SOUNDS ARE HEARD, OIL PRESSURE SHOULD BE PRESENT AND BOTH THE OIL PUMP AND ENGINE LUBRICATION SYSTEM ARE PRIMED. IF NO PRESSURE IS RECORDED, REPEAT STEP 3 THEN PROCEED TO STEP 7.

7. IF NO OIL PRESSURE IS RECORDED AFTER REPEATING PROCESS, REMOVE THE OIL FILTER ADAPTER AND FORCE ENGINE OIL UNDER PRESSURE (USING SHOP AIR) INTO THE ENGINE BLOCK OUTLET PORT **(THE PORT CLOSEST TO THE FRONT OF THE ENGINE.)** REINSTALL OIL FILTER ADAPTER AND RESTART ENGINE.

8. IF OIL PRESSURE IS OBTAINED, STOP ENGINE AND REINSTALL THE OIL PRESSURE SWITCH IN THE OIL FILTER ADAPTER. ONCE CONNECTED, CHECK THE INSTRUMENT PANEL DISPLAY FOR NO OIL PRESSURE OR "LOW OIL PRESSURE" MESSAGE. IF MESSAGE IS PRESENT, CHECK SWITCH CONNECTION OR CONSULT THE SERVICE MANUAL.

#### NOTE: WHENEVER SERVICING THE CONNECTING ROD AND/OR MAIN CRANKSHAFT BEARINGS, BE SURE TO APPLY A COAT OF LUBRIZOL(R), P/N 9780631 (CANADA P/N 992869), TO THE BEARING SURFACES AND CRANKSHAFT JOURNALS (COVER COMPLETELY). ALSO PERFORM THE FOLLOWING WHEN SERVICING THE INTERNAL COMPONENTS OF A 4.6L NORTHSTAR ENGINE; THESE STEPS WILL AID IN PRIMING THE SYSTEM.

- STORE THE VALVE LIFTERS WITH CAMSHAFT CONTACT SURFACE DOWN, SO ENGINE OIL WILL NOT DRAIN FROM THE LIFTERS.

- APPLY LIBERAL AMOUNTS OF LUBRIZOL(R), P/N 3530566 (CANADA P/N 992704), TO THE CAMSHAFT LOBES, BEARING CAPS AND LIFTER SURFACES. PISTON RINGS AND PISTONS SHOULD BE COMPLETELY COVERED WITH PROPER SPECIFICATION ENGINE OIL UPON INSTALLATION.

WE BELIEVE THIS SOURCE AND THEIR EQUIPMENT TO BE RELIABLE. THERE MAY BE ADDITIONAL MANUFACTURERS OF SUCH EQUIPMENT. GENERAL MOTORS DOES NOT ENDORSE, INDICATE ANY PREFERENCE FOR OR ASSUME ANY RESPONSIBILITY FOR THE PRODUCTS OR EQUIPMENT FROM THESE FIRMS OR FOR ANY SUCH ITEMS WHICH MAY BE AVAILABLE FROM OTHER SOURCES.

PLEASE INCLUDE THE ABOVE MENTIONED INFORMATION IN YOUR 1993 ALLANTE, SEVILLE AND ELDORADO SERVICE MANUALS.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.