SQUAWK NOISE FROM FRONT SUSPEN. (INST. NEW INSULATORS). Cadillac Allante 1991

For 1990-2009 cars

# SQUAWK NOISE FROM FRONT SUSPEN. (INST. NEW INSULATORS)

#### SUBJECT: SQUAWK NOISE FROM THE FRONT SUSPENSION (INSTALL NEW STABILIZER SHAFT INSULATORS)

#### MODELS: 1990-93 CADILLAC ALLANTE 1990-94 CADILLAC ELDORADO AND SEVILLE 1994 CADILLAC CONCOURS AND DEVILLE

********************************************************************** THIS BULLETIN CANCELS AND SUPERSEDES BULLETIN #313301. PREVIOUS DIVISIONAL PUBLICATION NUMBERS WERE: CADILLAC: T-93-103 AND GM OF CANADA: 93-3C-104. **********************************************************************

#### CONDITION:

SOME OWNERS MAY COMMENT ON A SQUAWK NOISE COMING FROM THE FRONT SUSPENSION DURING LARGE SUSPENSION TRAVEL (I.E., GOING THROUGH A DIP). THIS CONDITION IS MOST NOTICEABLE IN COLD TEMPERATURES AND MAY OCCUR ON ONLY THE FIRST FEW JOUNCES AFTER A COLD SOAK.

#### CAUSE:

THIS CONDITION IS CAUSED BY THE STABILIZER SHAFT ROTATING WITHIN THE STABILIZER SHAFT INSULATOR.

#### CORRECTION:

REPLACE THE STABILIZER SHAFT INSULATOR WITH THE NEW SERVICE PART THAT IS MADE FROM A DIFFERENT RUBBER COMPOUND. REFER TO THE SERVICE PARTS IDENTIFICATION LABEL FOR SUSPENSION OPTION CODE (FE1, FE2, OR FE3). THE INSULATORS SHOULD BE INSTALLED PER SERVICE INFORMATION MANUAL PROCEDURES WITH THE SLIT TOWARD THE REAR OF THE CAR.

YEAR SERIES SUSPENSION OPTION P/N 1990-1991 E FE1 3545378 E FE2 3545380 1992-1994 E FE1 3545376 E FE2 3545378 1993-1994 E FE3 3545380

1990-1994 K FE1 3545378 1990-1992 K FE2 3545380 1993-1994 K FE3 3545380

1994 KSP(DEVILLE) FE1 3545376 KSP(CONCOURS) FE1 3545378

1990-1993 V 3545378

IF THE SERVICE PARTS IDENTIFICATION LABEL IS NOT AVAILABLE, THE CORRECT INSULATOR PART NUMBER CAN BE DETERMINED BY MEASURING THE STABLIZER SHAFT DIAMETER ON INSULATOR SURFACE OR ON A CLEAN AREA OF THE SHAFT.

STABILIZER SHAFT INSTALL DIAMETER PART NUMBER ================ ===========

19MM 3545376 21MM 3545378 23MM 3545380

IF NEW BUSHING DOES NOT STAY SEATED PROPERLY OR WORKS OUT OF THE EXISTING BRACKET, INSTALL NEW BRACKETS, P/N 3547358 ON THE LEFT SIDE, AND P/N 3547359 ON THE RIGHT SIDE.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: E2180 LABOR TIME: .5 HR

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.